You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Node Status Report 0x0070

Node Status Report 0x0070

SwitchKit Name

NodeStatusReport

Type

EXS API and SwitchKit API message

Description

Node Status Report 0x0070

A CSP in a multi-node system sends this message to the host after the node reboots or its status changes.

Sent by

CSP

SwitchKit Code

C Structure

typedef struct {

int PhysicalNode;

UBYTE LogicalNode;

UBYTE HostNode;

UBYTE NodeStatus;

} XL_NodeStatusReport;

C++ Class

class XLC_NodeStatusReport : public XLC_InboundMessage {

public:

int getPhysicalNode() const;

void setPhysicalNode(int x);

UBYTE getLogicalNode() const;

void setLogicalNode(UBYTE x);

UBYTE getHostNode() const;

void setHostNode(UBYTE x);

UBYTE getNodeStatus() const;

void setNodeStatus(UBYTE x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length, MSB (0x0005)
3, 4 | Message Type (0x0070) | 3, 4 | Message Type (0x0070)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | 8 | Checksum
Number of AEs to follow
AE 0x11 Logical/Physical Span
: | Host Node ID The value is the same as the Logical Node ID field in the header. The system uses the value 0xF0 for a host node that does not have a logical node ID.
: | Node Status This field indicates the current status of the node. 0x00 Node Initialized 0x04 Multi Node System – ISUP Remote Control 0xFF Node Requires Logical Node ID
: | Checksum

A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
Most Significant Bit
See Address Information Block.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
See Integrated Services Digital Network User Part.