You are here: CSP Hardware Product Descriptions > 6 Resource Cards > Dialogic® Multi-Function Media I/O Plus Card - CSP-BIO-1400R

Dialogic® Multi-Function Media I/O Plus Card - CSP-BIO-1400R

Description

The Dialogic® Multi-Function Media I/O Plus card is required to provide Ethernet connectivity for the IP Network Interface Series 3 and DSP Series 2 Plus cards. This card connects to the IP Network Interface Series 2 and DSP Series 2 Plus cards through the chassis midplane.

Ethernet Ports

The Multi-Function Media I/O Plus card provides Ethernet ports for the following six 10/100 Base-T Ethernet auto-negotiating signals.

• Two Ethernet control signals that are available for redundant NFS.

• Of the four Ethernet data signals only data 0 port is available for RTP.

Placement

The Multi-Function Media I/O Plus card resides in the rear card slot of a CSP 2090, CSP 2110, or CSP 2040 chassis directly behind the corresponding IP Network Interface Series 2 or DSP Series 2 Plus card.

Configuration Information

The part number, serial number, model number, and revision are located on the back of the board.

Specifications

The Multi-Function Media I/O Plus card is designed to the following electrical, physical, and environmental specifications.

Electrical | Specification
--- | ---
Supply Voltage, Vcc | 5.00V
Supply Current, Vcc @ 5.0V | 1.0A (typical)

Physical | Specification
--- | ---
Height | 318.5 mm (12.54 in.)
Depth | 105.2 mm (4.14 in)
Width | 19.7 mm (0.775 in.)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

Model Number

The Multi-Function Media Plus I/O card model number is listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
Multi-Function Media Plus I/O | Not Applicable | CSP-BIO-1400R

Related Products

The products related to the Multi-Function Media I/O Plus card are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
DSP Series 2 Plus card with one module | Not Applicable | CSP-DSP-1410R
DSP Series 2 Plus card with two modules | Not Applicable | CSP-DSP-1420R

Front and Side Views

The front view shows the LEDs, push button switch, and Ethernet connectors.

Controls and Indicators

The table below describes the LEDs as shown in the front view of the Multi-Function Media I/O Plus card.

Fault, Hreset LEDs/Reset Push Button | Color/Status | Description
--- | --- | ---
Fault | Off | Reserved
Hreset | Green | Indicates the I/O card is being reset.
Reset | Initiates a reset of the I/O card.
Ethernet LEDs | Color/Status | Description
Activity | Green | Indicates both RX (receive) and TX (transmit) activity (20ms on time)
Off | Indicates no RX or TX activity
Col/FD (Collision/Duplex) | Green | Flashes when collision occurs in half duplex mode (20ms on time) Continuous indication when in full duplex mode Flashes (10 Hz) during continuous collisions
Off | Indicates no collisions
LNK (Link) | Green | Flashes during auto-negotiation Continuous indication when a link is established Continuously flashes during network misconfiguration
Off | Indicates loopback
100M (Speed) | Yellow | Indicates 100Base-T (100 Mbps) link established
Flashes (0.4 sec.) with no link established
Off | 10Base-T (10 Mbps) link not supported

The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
Digital Signal Processor
Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.
Hertz