You are here: CSP Hardware Product Descriptions > 7 Dialogic® CSP Expansion and Interconnect ONE I/O Card > EXNET® Fiber Optic Cable - See Part Numbers

EXNET® Fiber Optic Cable - See Part Numbers

Description

In a CSP, PCM data passes between nodes through the EXNET® ring, a proprietary 1.2 Gbps fiber optic network using a packet-based protocol. This section describes the physical aspects of the cable. Refer to the Hardware Installation and Maintenance Guide for complete CSP installation information.

Specifications

The cable supplied by Dialogic is a Duplex Zipcord fiber optic cable with the following specifications.

Parameter | Specification
--- | ---
Length | 1, 2 and 5 meters
Connectors | SC
Multi-mode | 850 nm
Fiber Size | 62.5/125 microns
Insertion Loss | 0.5 dB
Return Loss | Not Applicable

Cable Part Numbers

The EXNET® fiber optic cable part numbers are listed below.

Description | Part No. | RoHS Part No.
--- | --- | ---
EXNET-Multi-Mode Fiber Optic Cable, 1 meter | 16-5001-00 | 116-5001-00
EXNET-Multi-Mode Fiber Optic Cable, 2 meter | 16-5008-00 | 116-5008-00
EXNET-Multi-Mode Fiber Optic Cable, 5 meter | 16-5005-00 | 116-5005-00

Related Products

The products related to the EXNET® fiber optic cable are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
EXNET-ONE I/O Card | EXS-XIO-1200 | EXS-XIO-1200R

Fiber Optic Cable

The fiber optic cable is made up of the following components as shown below.

The nodes communicate by sending a laser beam signal over the fiber optic cable. Once the EXNET-ONE I/O card is installed and the laser beam is active, do not look into the EXNET® ports. You may damage your eyes.

If you install an EXNET-ONE I/O card without the fiber optic cable inserted in the EXNET® ports, insert the plastic I/O Port Plug in the ports.

Important! The EXNET Connect PCI H.100 card is not supported in Release 8.4.1. Refer to the CSP Technical Publications for Release 8.3.1 for information on this card.

See Pulse Code Modulation.
Excel's open architecture, proprietary, 1.3 Gbps fiber optic network using a packet-based protocol.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
Peripheral Component Interconnect