0x01AE Poll Interval Configure

Use this TLV to specify the poll interval and the number of missed polls before a connection is declared down.

Used in:
VoIP Protocol Query message
VoIP Protocol Configure message

Byte | Description
0, 1 | Tag 0x01AE
2, 3 | Length 0x0004
4 | Value[0] Poll Interval, MSB: 0x00-0xFF
5 | Value[1] Poll Interval, LSB: 0x00-0xFF
6 | Value[2] Number of Missed Polls Before Link is Declared Down, MSB: 0x00-0xFF
7 | Value[3] Number of Missed Polls Before Link is Declared Down, LSB: 0x00-0xFF

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Most Significant Bit
Least Significant Bit