You are here: CSP Developer’s Guide: Overview > 8 DSP Series 2 Cards Product Description > Hardware

Hardware

Compatibility

The DSP Series 2 card may reside in an CSP that also contains DSP-ONE cards, and the platform can pool identical resources from these cards and use them together.

The 2090 chassis can accept a maximum of five DSP Series 2 cards, while the 2040 chassis can accept a maximum of two DSP Series 2 cards.

The DSP Series 2 card may not reside in an CSP that also contains MFDSP cards.

I/O

The DSP Series 2 card requires a Multi-Function Media I/O card for File Record/Playback and Fax functionality.

Modules and DSPs

The DSP Series 2 card comes with either one or two DSP 2 Modules with four DSPs each, for a maximum of eight DSPs per card.

Figure 8-1 Modules on the DSP Series 2 Card

Digital Signal Processor