0x55 Conference ID

Use this AE with the Slot AE (unless noted) in the following messages:

Play File Start

Play File Stop

Play File Modify

Record File Start

Record File Stop

Record File Modify

System Configuration Query (no Slot AE)

Generic Report (no Slot AE)

Byte | AIB Field Description
--- | ---
2 | Address Element: 0x55 Conference ID
3 | Data Length: 0x02
4, 5 | Data[0, 1]: Conference ID (MSB, LSB)

See Address Information Block.
The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.
Most Significant Bit
Least Significant Bit