# 3 Line Cards

Purpose

This chapter provides descriptions of the Network Interface Line cards.

Compliance

The Network Interface Line cards comply with all relevant regulations from the following standards organizations and governing bodies.

Country/Standards Organization | Regulations
--- | ---
United States and Canada | FCC Part 15 and ICES 003 CSA C22.2 No. 60950-1-3 CB Scheme IEC 60950-1 Telecom FCC Part 68/IC CS03/T1.102
NEBS | NEBS Level 3 (GR-1089-CORE, GR-63-CORE)
European Union (CE Mark) | EN 55022: 1998/A1:2000/A2:2003 EN 55024: 1998/A1:2000/A2:2003 EN 300 386: Version 1.3.3 EN 60950-1 Telecom TBR 4, 12, 13, G.703 NTR 11 Compliant • DPNSS/DASS2 package includes the E-ONE 75 Ohm interfaces. NTR 4 Compliant • E-ONE 75 Ohm LC, E-ONE 75 Ohm I/O, E-ONE 75 Ohm Redundant I/O, E-ONE 75 Ohm Standby I/O
Australia/New Zealand | AS/NZS CISPR 22:2002 AS/NZ 60950-1 Telecom AS/ACIF S-016 and S-038

In this section:

Dialogic® DS3 Card - CSP-DS3-1001R

Dialogic® DS3 I/O Card - EXS-DS3-1100/EXS-DS3-1100R

Dialogic® Standby DS3 I/O Card - EXSDIO1200/EXSDIO1200R

DS3 Cable Assembly - Part Nos. 64-0124-00/164-0124-00

Dialogic® E-ONE Card - See Model Numbers

Dialogic® E-ONE 120 Ohm I/O Card - EXSEIO1000/EXSEIO1000R

Dialogic® E-ONE 120 Ohm Red I/O Card - EXSEIO1200/EXSEIO1200R

Dialogic® E-ONE 120 Ohm Standby I/O Card - EXS-EIO-1300/ EXS-EIO-1300R

Dialogic® E-ONE 75 Ohm I/O Card - EXSEIO1010/EXSEIO1010R

Dialogic® E-ONE 75 Ohm Red I/O Card - EXSEIO1210/EXSEIO1210R

Dialogic® E-ONE 75 Ohm Standby I/O Card - EXSEIO1310/EXSEIO1310R

Dialogic® J-ONE Card - See Model Numbers

Dialogic® J-ONE Redundant I/O Card - EXSJIO1200

Dialogic® J-ONE Standby I/O Card - EXSJIO1300

Dialogic® T-ONE Card - See Model Numbers

Dialogic® T-ONE 100 Ohm I/O Card - EXSTIO1000/EXSTIO1000R

Dialogic® T-ONE 100 Ohm Red I/O Card - EXSTIO1200/EXSTIO1200R

Dialogic® T-ONE 100 Ohm Standby I/O Card - EXSTIO1300/EXSTIO1300R

Telco Cable Assembly - See Part Numbers

See Converged Services Administrator.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
See Application Server.