ISUP CQS Configuration Bytes (ANSI)

Byte | Description | Value
--- | --- | ---
0x01 | Max Range | 31
0x02 | Recovery Action (as defined by ANSI T1.113) should be taken if this byte is set to 0x01. | 0x00=Do Not Perform Auto-Recovery 0x01=Perform Auto-Recovery
0x03 | Circuit State Indicator Parameter ID | 0x26 (Circuit State Indicator)
Release (REL) for Protocol Error
0x0A | Information Length | 0x06
0x0B | Message ID | 0x0C (REL)
0x0C | Parameter Count | 0x01
0x0D | Parameter 1 ID | 0x12 (Cause Indicators)
0x0E | Parameter 1 Data Length | 0x02
0x0F | Parameter 1 Data[0] | 0x80 (Location=User)
0x10 | Parameter 1 Data[1] | 0xEF (Cause 111=Protocol Error, Unspecified)

American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.