SSUTR2 CPC Configuration Bytes

Byte | Description | Value
--- | --- | ---
0x0A | LIG (Release Guard Field Count) | 0
0x14 | ECH (Call Failure Signal Field Count) | 0
0x19 | Specialized Circuit (Location of this byte must not be changed) | 0=Mixed circuit (incoming/outgoing) (default) 1=Outgoing call only
0x1A | Congestion Control Enabled/Disabled | 0=Disabled 1=Enabled (default)
0x1B | Congestion Signal Type | 1=EEC 2=EFC 3=ERN
0x1E | FIU (Clear Forward Field Count) | 0