0x9041 Protocol Parameters

Use this TLV to either:

• assign the default standard and network identity

or

• create maps and assign the values for standard and network identity to the maps

Used in:
NGA Configure message

Byte | Description
0, 1 | Tag 0x9041
2, 3 | Length 0x0015
4-7 | Value[0-3] Default Standard 0x00 - M3UA Stack ANSI 0x01 - M3UA Stack ITU
8-11 | Value [4-7] Default Network Identity 0x00 - M3UA NW International 0x01 - M3UA NW National No. Priority 0x02 - M3UA NW National Priority 0x03 - M3UA NW Invalid
12 | Value [8] Number of Maps
13-16 | Value[9-12] Network Appearance 4-byte number unique in the network
17-20 | Value[13-16] Standard 0x00 - M3UA Stack ANSI 0x01 - M3UA Stack ITU
21-24 | Value [17-20] Network Identity 0x00 - M3UA NW International 0x01 - M3UA NW National No. Priority 0x02 - M3UA NW National Priority 0x03 - M3UA NW Invalid

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
International Telecommunications Union (UN)