0x05FD CPU Statistics

This TLV may be included in the response to the Statistics Query message.

Byte | Description
0, 1 | Tag: 0x05FD CPU Statistics
2, 3 | Length: 0x0034
4 | Value[0]: DSP Module
5 | Value[1]: DSP Chip
6 | Value[2]: Percentage Idle
7 | Value[3]: Percentage of time in the kernel task
8 | Value[4]: Percentage of time in servicing interrupts
9 | Value[5]: Percentage of time in the tnettask task
10 | Value[6]: Percentage of time in the tdspx task
11 | Value[7]: Percentage of time in the tdspr task
12 | Value[8]: Percentage of time in the tnet task
13 | Value[9]: Percentage of time in the trac task
14 | Value[10]: Percentage of time in the tvrap task
15 | Value[11]: Total percentage of time
16-19 | Value[12-15]: Number of ticks idle
20-23 | Value[16-19]: Number of ticks in the kernel task
24-27 | Value[20-23]: Number of ticks in servicing interrupts
28-31 | Value[24-27]: Number of ticks in the tnettask task
32-35 | Value[28-31]: Number of ticks in the tdspx task
36-39 | Value[32-35]: Number of ticks in the tdspr task
40-43 | Value[36-39]: Number of ticks in the tnettask task
44-47 | Value[40-43]: Number of ticks in the trac task
48-51 | Value[44-47]: Number of ticks in the tvrap task
52-55 | Value[48-51]: Total ticks

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor