You are here: CSP Developer’s Guide: Line Cards > 2 T1 Information > T1 Call Setup

T1 Call Setup

Tables E&M through FXO/GS show the ICB subtypes that are supported for each T1 protocol in these API messages:

• Inseize Instruction List Configure

• Outseize Instruction List Configure

• Inseize Control

• Outseize Control

Table 2-3 E&M

Outgoing | Incoming
--- | ---
The only valid outseize control Action ICBs used for the default E&M protocol are the following: | The only valid inseize control Action ICBs used for the default E&M protocol are the following:
0x00 Null | 0x00 Null
0x01 Scan for Wink N | 0x01 Report Call Processing Event
0x02 Scan for ANI Request Off-hook | 0x02 Generate Call Processing Event
0x04 Report Call Processing Event | 0x03 Receive Stage N Address Data
0x05 Outpulse Stage N Address Data | 0x04 Wait for Host Control
0x06 Wait for Host Address Data | 0x05 Report Incoming Call
0x07 Wait for Host Control | 0x06 Report Incoming Call with Digits
0x08 Send Host Acknowledgment | 0x07 Generate Inseize Acknowledgment
0x09 Do Call Progress Analysis | 0x08 Send Host Acknowledgment
0x0A Seize | 0x09 Use Instruction List
0x0B Use Instruction List | 0x0A Delay N ms
0x0F Wait for Host control with Answer |
0x10 Do CPA Without Line Signaling |
0x11 Delay N ms |

Table 2-4 FXS/LS

Outgoing | Incoming
--- | ---
The only valid outseize control Action ICBs used for the default FXS/LS protocol are the following: | The only valid inseize control Action ICBs used for the default FXS/LS protocol are the following:
0x00 Null | 0x00 Null
0x07 Wait for Host Control | 0x01 Report Call Processing Event
0x08 Send Host Acknowledgment | 0x03 Receive Stage N Address Data
0x0A Seize | 0x04 Wait for Host Control
0x0B Use Instruction List | 0x05 Report Incoming Call
0x0F Wait for Host control with Answer | 0x06 Report Incoming Call with Digits
0x11 Delay N ms | 0x07 Generate Inseize Acknowledgment
| 0x08 Send Host Acknowledgment
| 0x09 Use Instruction List
| 0x0A Delay N ms

Table 2-5 FXO/LS

Outgoing | Incoming
--- | ---
The only valid outseize control Action ICBs used for the default FXO/LS protocol are the following: | The only valid inseize control Action ICBs used for the default FXO/LS protocol are the following:
0x00 Null | 0x00 Null
0x03 Scan for Dial Tone | 0x04 Wait for Host Control
0x04 Report Call Processing Event | 0x05 Report Incoming Call
0x05 Outpulse Stage N Address Data | 0x07 Generate Inseize Acknowledgment
0x06 Wait for Host Address Data | 0x08 Send Host Acknowledgment
0x07 Wait for Host Control | 0x09 Use Instruction List
0x08 Send Host Acknowledgment | 0x0A Delay N Milliseconds
0x09 Do Call Progress Analysis |
0x0A Seize |
0x0B Use Instruction List |
0x0F Wait for Host Control with Ans |
0x11 Delay N Milliseconds |

Table 2-6 FXS/GS

Outgoing | Incoming
--- | ---
The only valid outseize control Action ICBs used for the default FXS/GS protocol are the following: | The only valid inseize control Action ICBs used for the default FXS/GS protocol are the following:
0x00 Null | 0x00 Null
0x07 Wait for Host Control | 0x01 Report Call Processing Event
0x08 Send Host Acknowledgment | 0x03 Receive Stage N Address Data
0x0A Seize | 0x04 Wait for Host Control
0x0B Use Instruction List | 0x05 Report Incoming Call
0x0F Wait for Host Control with Answer | 0x06 Report Incoming Call with Digits
0x11 Delay N ms | 0x07 Generate Inseize Acknowledgment
| 0x08 Send Host Acknowledgment
| 0x09 Use Instruction List
| 0x0A Delay N ms

Table 2-7 FXS/GS

Outgoing | Incoming
--- | ---
The only valid outseize control Action ICBs used for the default FXS/GS protocol are the following: | The only valid inseize control Action ICBs used for the default FXS/GS protocol are the following:
0x00 Null | 0x00 Null
0x07 Wait for Host Control | 0x01 Report Call Processing Event
0x08 Send Host Acknowledgment | 0x03 Receive Stage N Address Data
0x0A Seize | 0x04 Wait for Host Control
0x0B Use Instruction List | 0x05 Report Incoming Call
0x0F Wait for Host Control with Answer | 0x06 Report Incoming Call with Digits
0x11 Delay N ms | 0x07 Generate Inseize Acknowledgment
| 0x08 Send Host Acknowledgment
| 0x09 Use Instruction List
| 0x0A Delay N ms

Table 2-8 FXO/GS

Outgoing | Incoming
--- | ---
The only valid outseize control Action ICBs used for the default FXO/GS protocol are the following: | The only valid inseize control Action ICBs used for the default FXO/GS protocol are the following:
0x00 Null | 0x00 Null
0x03 Scan for Dial Tone | 0x04 Wait for Host Control
0x04 Report Call Processing Event | 0x05 Report Incoming Call
0x05 Outpulse Stage N Address Data | 0x07 Generate Inseize Acknowledgment
0x06 Wait for Host Address Data | 0x08 Send Host Acknowledgment
0x07 Wait for Host Control | 0x09 Use Instruction List
0x08 Send Host Acknowledgment | 0x0A Delay N ms
0x09 Do Call Progress Analysis |
0x0A Seize |
0x0B Use Instruction List |
0x0F Wait for Host Control with Answer |
0x11 Delay N ms |

See Information Control Block.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
Outgoing call setup during real-time call processing on a specific channel.
Incoming call setup during real time call processing on a specific channel.
Momentary interruption in a single frequency tone indicating the distant switch is ready to receive the digits just dialed.
See Automatic Number Identification.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
See Loop Start.