0x068C FAX Page Range

Use this TLV in the Resource Connect (0x0127) message to specify a page range for FAX transmission.

• To FAX a single page, enter same page number for Start Page and End Page.

• If the page range specified extends beyond the end of the TIFF file, the file will be transmitted to completion from the specified start page.

• If the specified start page is beyond the end of the TIFF file, then a Fax complete event shall be generated and no pages shall be transmitted.

Byte | Description
0, 1 | Tag: 0x068C FAX Page Range
2, 3 | Length: 0x0004
4, 5 | Start Page Default = 0x01
6, 7 | End Page Default = End of File

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.