0x66 SS7 Address Information

Used in:
Request for Service with Data message
Outseize Control message

ICB Type | 0x02 (Data)
ICB ID | 0x66
Data Length | 0x0C
Data[0-3] | CIC (4 Bytes)
Data[4-7] | OPC (4 Bytes)
Data[8-11] | DPC (4 Bytes)

Outgoing call setup during real-time call processing on a specific channel.
See Information Control Block.
See Circuit Identification Codes.
Destination Point Code