0x2A0B Media Clock Rate

Used in:
0x0033 NPDI Universal ICB

Byte | Description
0, 1 | Tag 0x2A0B
2, 3 | Length 0x0004
4-7 | Value[0-3] Clock Rate

Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.