You are here: CSP Hardware Product Descriptions > 1 Chassis > CSP 2110 Fan Tray, Front - EXSFTL0111/EXSFTL0111R

CSP 2110 Fan Tray, Front - EXS-FTL-0111/EXS-FTL-0111R

Description

The front fan tray and rear fan tray, as shown below, are both required to ensure proper air flow and cooling of the CSP 2110 chassis. The front fan tray is powered by the -48 V DC midplane bus. It can be removed with the power on. The front fan tray provides an air filter to remove particulate accumulation.

Air Filter

The air filter must be replaced periodically to remove particulate accumulation. Preventive maintenance schedules will vary depending on the chassis’s environmental conditions. Refer to the Hardware Installation and Maintenance Guide, for filter removal and replacement procedures.

Configuration Information

The part number, serial number, model number, and revision are located on the back of the fan tray.

Specifications

The front fan tray is designed to the following electrical, physical and environmental specifications.

Electrical | Specification
--- | ---
Input Power Requirement | -48 V DC
Input Voltage Range | -40 V DC to -60 V DC

Physical | Specification
--- | ---
Height | 5.7 cm (2.25 in.)
Width | 42.5 (16.75 in.)
Depth | 31.7 cm (12.5 in.)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

Related Products

The products related to the CSP 2110 front fan tray are listed below

Product | Model No. | RoHS Model No.
--- | --- | ---
CSP 2110 Chassis | EXS-CHA-1201 | EXS-CHA-1201R

Fan Tray Locations

This shows the location of the fan trays.

Front Fan Tray Components

The front fan tray components are shown below.