L3P BT IUP Configuration Bytes

Block 1

The L3P BT IUP configuration bytes below are included in Block 1.

Byte | Description of Block 1 Byte | Value
--- | --- | ---
0x01 | Generate PPL Event Indication for IAM Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x02 | Generate PPL Event Indication for IFAM Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x03 | Generate PPL Event Indication for SAM Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x04 | Generate PPL Event Indication for FAM Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x05 | Generate PPL Event Indication for Send "N" Digits Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x06 | Generate PPL Event Indication for Send All Digits Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x07 | Generate PPL Event Indication for Send Additional Setup Information Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x08 | Generate PPL Event Indication for Address Complete Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x09 | Generate PPL Event Indication for Congestion Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x0A | Generate PPL Event Indication for Terminal Congestion Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x0B | Generate PPL Event Indication for Connection Not Admitted Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x0C | Generate PPL Event Indication for Repeat Attempt Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x0D | Generate PPL Event Indication for Subscriber Engaged Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x0E | Generate PPL Event Indication for Subscriber Out of Order Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x0F | Unused |
0x10 | Unused |
0x11 | Generate PPL Event Indications for Answer Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x12 | Generate PPL Event Indication for Clear Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x13 | Generate PPL Event Indication for Re-Answer Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x14 | Generate PPL Event Indication for Release Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x15 | Unused |
0x16 | Unused |
0x17 | Unused |
0x18 | Unused |
0x19 | Generate PPL Event Indications for Circuit Free Bit Number Message 0 Generate State 2-7 Unused | Note 2 0 (default)
0x1A | Generate PPL Event Indication for Blocking Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x1B | Generate PPL Event Indication for Unblocking Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x1C | Generate PPL Event Indication for Block Ack Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x1D | Generate PPL Event Indication for Unblock Ack Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x1E | Generate PPL Event Indication for Overload Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x1F | Unused |
0x20 | Unused |
0x21 | Unused |
0x22 | Unused |
0x23 | Unused |
0x24 | Unused |
0x25 | Generate PPL Event Indication for Confusion Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x26 | Generate PPL Event Indication for ISDN Composite Service Info Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x27 | Unused |
0x28 | Unused |
0x29 | Generate PPL Event Indications for Additional Call Information Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x2A | Unused |
0x2B | Unused |
0x2C | Generate PPL Event Indication for Swap Bit Number Message 0 Generate State 2-7 Unused | See Note 2. 0 (default)
0x2D | For the AUTO (IAM-SND) protocol: The number of accumulated digits received must be greater than or equal to this value to prevent another SND message from being sent. For the AUTO (IAM-SAD) protocol: The number of accumulated digits received must be greater than or equal to this value to prevent another SAD message from being sent. See config block 1, byte 0x2E for setting of the AUTO (IAM-SND) or AUTO (IAM-SAD) modes. NOTE: If more than 30 digits are received the channel will be purged. | 0 = Default
0x2E | IAM Operational Mode. Auto(IAM-SND)/Host/AUTO(IAM-SAD) control of messaging on reception of an IAM. In Auto IAM-SND Mode the PPL code will automatically attempt to retrieve the Desires number of Digits based upon the setting in the above config byte using the SND protocol. In Host mode the Host must request any desired additional digits, and ACI messages, if required. It must deal with the networks responses appropriately. In the AUTO IAM-SAD mode the PPL code will automatically attempt to retrieve at least the desired number of digits based upon the setting in the above config byte or timer 0x16 expiring or the reception of a FAM using the SAD protocol. | 0 = Default AUTO IAM-SND 1 = Host CTRL 2 = AUTO IAM-SAM
0x2F | IFAM Operational Mode. This controls the PPL processing by selection of one of two actions. L3p takes these actions after the IFAM is received and a Setup message is sent to L4. In the Basic processing mode, the PPL waits for L4 to issue an Alerting message, or any other Host desired message wrapped in a PPL Event Request. In the Auto mode, the PPL will issue an ACI/ASUI message to L3 and await it’s response. Once received it will send a PPL Event Indication of ACI/ASUI to the Host. ACI is sent whenever the received Interworking bit in the IAM/IFAM message, is zero and ASUI when the bit is a one. The ACI/ASUI responses will be generated by the PPL code whenever a valid request is received regardless of this config byte’s setting. Auto response to ACI request messages. PNI processing. When enabled, and the PNI bit is set will cause up to 2 Auto ACI requests to be issued. As defined in config block 1 bytes 0x60 and 0x61. | Bit 0 0 = Default, Auto ACI/ASUI 1 = Basic Bit 1 0 = Default, Auto respond to ACI request. 1 = Do not respond automatically to ACI request. Allow Host to respond. Bit 2 0 = Disabled 1 = Enabled
0x30 | L3p IUP Setup Report Format. Bit Number Message 0 ICB encoding to use whenever L3pIUP is required to issue a Setup msg to L4. 1-7 Unused | 0, Report using actual IUP ICBs = Default. 1, Report only the called address (optionally calling address) using Stage N Address Data ICB in BCD.
0x31 | Network Configuration Bit Number Description 0 Unused 1 Unidirectional/Both way. 2 Exchange Type | 0 = Default, Both way 1= Unidirectional 0 = Terminating 1 = Intermediate
0x32 | Out Of Service to Inservice transition notification. 0 = Send UBL (Unblock) to network 1 = Send nothing | 0 = Default
0x33 | Control Reporting of Call Connected upon receiving ANS. 0 = Suppress Message 1 = Issue PPL Event Indication message | 1 = Default
0x34 | The RFS with data will not be reported to the HOST until after the results of the ACI/SASUI is collected. The Host will be presented with a single IUP ICB containing the original IAM/IFAM message and the received ACI/SASUI response. When this byte is set, config block 1, byte 0x2F is ignored, but it’s functionality is activated to get the ACI/ASUI responses | 0 = Default Disable late RFS reporting. 1 = Enable RFS reporting after auto ACI request/response.
0x35 | Outgoing Congestion Control | 0= Enabled- Default. 1 = Disabled.
0x36 | For the AUTO (IAM-SND) or AUTO (IAM-SAD) protocol: The Minimum number of accumulated digits when a FAM is received. If this minimum is not satisfied the call will be denied via a CAN. Use config block 1, byte 0x2D to set the minimum number of IAM/SAM digits to receive. | 0 = Default
0x37 | Number of digits to match. If these digits match the digits in the accumulated digit buffer then use the value in config block 1, byte 0x3D in stead of config byte 0x2D to limit the number of SNDs/SADs to issue. And use the value in config block 1, byte 0x3E in stead of config byte 0x36 to set the minimum number of digits required when a FAM is received. | 0 = Default
0x38 | First two digits to match | 0 = Default
0x39 | Second two digits to match | 0 = Default
0x3A | Third two digits to match | 0 = Default
0x3B | Fourth two digits to match | 0 = Default
0x3C | Fifth two digits to match | 0 = Default
0x3D | Alternate minimum number of digits that must be received to prevent another SND or SAD to be issued. Used instead of config block 1, byte 0x2D. | 0 = Default
0x3E | Alternate minimum number of digits that must be received to successfully allow a FAM to complete the address information. Used in stead of config block 1, byte 0x36. | 0 = Default
0x3F | If PPL Event Request of ANM is sent to L3P to automatically put, L4 in the answer state. | 0 - Do not put L4 in answered state automatically (default) 1 - Put L4 in answered state automatically
0x40-0x5F | Unused |
0x60 | When PNI processing is enabled, The Auto ACI IRC value to be used when the PNI bit is clear, or the second Auto ACI IRC value to be used when the PNI is set. When PNI processing is disabled this contains the Auto ACI IRC value. | 0 = Don’t issue Request. 1 = Default
0x61 | When PNI processing is enabled, The first Auto ACI IRC value to be used when the PNI bit is set. | 0 = Don’t issue Request. 0 = Default
0x62 | Preserve Block states when DPC becomes inaccessible. | 0 = Preserve 1 = Destroy
0x63 | Preserve (Maintain) Answered Calls when DPC becomes inaccessible. | 0 = Preserve 1 = Destroy
0x64 | Beginning of IAM Message. Number of TLVs that follow | 4
0x65 | H0 H1 element TLV ID | 1
0x66 | Length of TLV data to follow | 2
0x67 | First byte (i.e. H0) of H0 H1 | 0
0x68 | Second byte (i.e. H1) of H0 H1 | 0
0x69 | IAM/IFAM Message Ind. TLV ID | 2
0x6A | Length of TLV data to follow | 5
0x6B-0x6F | Data for this TLV |
0x70 | Called Address TLV ID | 3
0x71 | Length of TLV data to follow | Variable 2 to 0x0B, 0x0B = Default
0x72-0x7C | Data for this TLV |
0x7D | Line Identity TLV | 4
0x7E | Length of TLV data to follow | Variable 2 to 9, 9 = Default
0x7F-0x87 | Data for this TLV |
0x88 | Beginning of IFAM Message. Number of TLVs that follow | 4
0x89 | H0 H1 element TLV ID | 1
0x8A | Length of TLV data to follow | 2
0x8B-0x8C | Data for this TLV |
0x8D | IAM/IFAM Message Ind. TLV ID | 2
0x8E | Length of TLV data to follow | 5
0x8F-0x93 | Data for this TLV |
0x94 | Called Address TLV ID | 3
0x95 | Length of TLV data to follow | variable 2 to 0x0B, 0x0B = Default
0x96-0xA0 | Data for this TLV |
0xA1 | Line Identity TLV ID | 4
0xA2 | Length of TLV data to follow | variable 2 to 9, 9 = Default
0xA3-0xAB | Data for this TLV |
0xAC | Beginning of SAM Message. Number of TLVs that follow | 2
0xAD | H0 H1 element TLV ID | 1
0xAE | Length of TLV data to follow | 2
0xAF-0xB0 | Data for this TLV |
0xB1 | Reserved Data Byte TLV ID | 0x18
0xB2 | Length of TLV data | 1
0xB3 | Reserved byte | 0
0xB4 | SAM/FAM Called Address TLV ID | 0x19
0xB5 | Length of TLV data to follow | variable 2 to 0x0A, 0x0A = Default
0xB6-0xBF | Data for this TLV |
0xC0 | Beginning of FAM Message. Number of TLVs that follow | 2
0xC1 | H0 H1 element TLV ID | 1
0xC2 | Length of TLV data to follow | 2
0xC3-0xC4 | Data for this TLV |
0xC5 | Reserved Data Byte TLV ID | 0x18
0xC6 | Length of TLV data | 1
0xC7 | Reserved byte | 0
0xC8 | SAM/FAM Called Address TLV ID | 0x19

Block 2

The L3P BT IUP configuration bytes below are included in Block 2.

Byte | Description of Block 2 Byte | Value
--- | --- | ---
0x01 | Length of TLV data to follow | variable 2 to 0x0A, 0x0A = Default
0x02-0x0B | Data for this TLV |
0x0C | Beginning of ASUI Type 1 Message. Number of TLVs that follow | 3
0x0D | H0 H1 element TLV ID | 1
0x0E | Length of TLV data to follow | 2
0x0F-0x10 | Data for this TLV |
0x11 | ASUI Message Information Contained Code TLV ID | 5
0x12 | Length of TLV data to follow | 1
0x13 | Data for this TLV | 0
0x14 | Line Identity TLV ID | 4
0x15 | Length of TLV data to follow | Variable 2 to 9, 9 = Default
0x16-0x1E | Data for this TLV |
0x1F | Beginning of ASUI Type 2 Message. Number of TLVs that follow | 4
0x20 | H0 H1 element TLV ID | 1
0x21 | Length of TLV data to follow | 2
0x22-0x23 | Data for this TLV |
0x24 | ASUI Message Information Contained Code TLV ID | 5
0x25 | Length of TLV data to follow | 1
0x26 | Data for this TLV | 0
0x27 | Reserved Data Byte TLV ID | 0x18
0x28 | Length of TLV data to follow | 1
0x29 | Data for this TLV | 0
0x2A | Partial Calling Line Identity TLV ID | 6
0x2B | Length of TLV data to follow | Variable 2 to 9, 9 = Default
0x2C-0x34 | Data for this TLV |
0x35 | Beginning of SND Message. Number of TLVs that follow | 2
0x36 | H0 H1 element TLV ID | 1
0x37 | Length of TLV data to follow | 2
0x38-0x39 | Data for this TLV |
0x3A | Number of Digits Requested TLV ID | 7
0x3B | Length of TLV data to follow | 1
0x3C | Data for this TLV | 0
0x3D | Beginning of SAD Message. Number of TLVs that follow | 2
0x3E | H0 H1 element TLV ID | 1
0x3F | Length of TLV data to follow | 2
0x40-0x41 | Data for this TLV |
0x42 | Reserved Data Byte TLV ID | 0x18
0x43 | Length of TLV data to follow | 1
0x44 | Reserved byte | 0
0x45 | Beginning of SASUI Message. Number of TLVs that follow | 2
0x46 | H0 H1 element TLV ID | 1
0x47 | Length of TLV data to follow | 2
0x48-0x49 | Data for this TLV |
0x4A | SAUSI Information Indicator TLV ID | 8
0x4B | Length of TLV data to follow | 1
0x4C | Data for this TLV |
0x4D | Beginning of ACM Message. Number of TLVs that follow | 2
0x4E | H0 H1 element TLV ID | 1
0x4F | Length of TLV data to follow | 2
0x50-0x51 | Data for this TLV |
0x52 | Address Complete Message Indicator TLV ID | 9
0x53 | Length of TLV data to follow | 3
0x54-0x56 | Data for this TLV |
0x57 | Beginning of CNG Message. Number of TLVs that follow | 1
0x58 | H0 H1 element TLV ID | 1
0x59 | Length of TLV data to follow | 2
0x5A-0x5B | Data for this TLV |
0x5C | Beginning of TCM Message. Number of TLVs that follow | 1
0x5D | H0 H1 element TLV ID | 1
0x5E | Length of TLV data to follow | 2
0x5F-0x60 | Data for this TLV |
0x61 | Beginning of CAN Message. Number of TLVs that follow | 3
0x62 | H0 H1 element TLV ID | 1
0x63 | Length of TLV data to follow | 2
0x64-0x65 | Data for this TLV |
0x66 | CAN Reason TLV ID | 0x0A
0x67 | Length of TLV data to follow | 1
0x68 | Data for this TLV |
0x69 | CAN Diagnostics TLV ID | 0x0B
0x6A | Length of TLV data to follow | 1
0x6B | Data for this TLV |
0x6C | Beginning of ANS Message. Number of TLVs that follow | 2
0x6D | H0 H1 element TLV ID | 1
0x6E | Length of TLV data to follow | 2
0x6F-0x70 | Data for this TLV |
0x71 | Type of Answer TLV ID | 0x0B
0x72 | Length of TLV data to follow | 1
0x73 | Data for this TLV |
0x74 | Beginning of CLR Message. Number of TLVs that follow | 1
0x75 | H0 H1 element TLV ID | 1
0x76 | Length of TLV data to follow | 2
0x77-0x78 | Data for this TLV |
0x79 | Beginning of REL Message. Number of TLVs that follow | 2
0x7A | H0 H1 element TLV ID | 1
0x7B | Length of TLV data to follow | 2
0x7C-0x7D | Data for this TLV |
0x7E | Release Reason TLV ID | 0x0D
0x7F | Length of TLV data to follow | 1
0x80 | Data for this TLV | 0x2F
0x81 | Beginning of CCF Message. Number of TLVs that follow | 1
0x82 | H0 H1 element TLV ID | 1
0x83 | Length of TLV data to follow | 2
0x84-0x86 | Data for this TLV |
0x86 | Beginning of BLO Message. Number of TLVs that follow | 1
0x87 | H0 H1 element TLV ID | 1
0x88 | Length of TLV data to follow | 2
0x89-0x8A | Data for this TLV |
0x8B | Beginning of UBL Message. Number of TLVs that follow | 1
0x8C | H0 H1 element TLV ID | 1
0x8D | Length of TLV data to follow | 2
0x8E-0x8F | Data for this TLV |
0x90 | Beginning of BLA Message. Number of TLVs that follow | 1
0x91 | H0 H1 element TLV ID | 1
0x92 | Length of TLV data to follow | 2
0x93-0x94 | Data for this TLV |
0x95 | Beginning of UBA Message. Number of TLVs that follow | 1
0x96 | H0 H1 element TLV ID | 1
0x97 | Length of TLV data to follow | 2
0x98-0x99 | Data for this TLV |
0x9A | Beginning of CFN Message. Number of TLVs that follow | 2
0x9B | H0 H1 element TLV ID | 1
0x9C | Length of TLV data to follow | 2
0x9D-0x9E | Data for this TLV |
0x9F | Confusion Message Qualifier TLV ID | 0x0E
0xA0 | Length of TLV data to follow | 1
0xA1 | Data for this TLV |
0xA2 | Beginning of ACI Type 1 Message. Number of TLVs that follow | 5
0xA3 | H0 H1 element TLV ID | 1
0xA4 | Length of TLV data to follow | 2
0xA5-0xA6 | Data for this TLV |
0xA7 | ACI Information Contained and Information Requested TLV ID | 0x0F
0xA8 | Length of TLV data to follow | 2
0xA9-0xAA | Data for this TLV |
0xAB | ACI Type 1 Reserved Bytes TLV ID | 0x10
0xAC | Length of TLV data to follow | 2
0xAD-0xAE | Data for this TLV |
0xAF | ACI Type 1 Message Indicators TLV ID | 0x11
0xB0 | Length of TLV data to follow | 1
0xB1 | Data for this TLV |
0xB2 | Line Identity TLV ID | 4
0xB3 | Length of TLV data to follow | variable 2 to 9, 9 = Default
0xB4-0xBC | Data for this TLV |
0xBD | Beginning of ACI Type 2 Message. Number of TLVs that follow | 3
0xBE | H0 H1 element TLV ID | 1
0xBF | Length of TLV data to follow | 2
0xC0-0xC1 | Data for this TLV |
0xC2 | ACI Information Contained and Information Requested TLV ID | 0x0F
0xC3 | Length of TLV data to follow | 2
0xC4-0xC5 | Data for this TLV |
0xC6 | Partial Calling Line Identity TLV ID | 6
0xC7 | Length of TLV data to follow | Variable 2 to 9, 9 = Default
0xC8 | Data for this TLV |

Block 3

The L3P BT IUP configuration bytes below are included in Block 3.

| Description for Block 3 Byte | Value
--- | --- | ---
1-8 | Data for last byte of this TLV |
9 | Beginning of ACI Type 3 Message. Number of TLVs that follow | 5
0x0A | H0 H1 element TLV ID | 1
0x0B | Length of TLV data to follow | 2
0x0C-0x0D | Data for this TLV |
0x0E | ACI Information Contained and Information Requested TLV ID | 0x0F
0x0F | Length of TLV data to follow | 2
0x10-0x11 | Data for this TLV |
0x12 | Calling/Called Subscriber’s Basic Service Marks TLV ID | 0x12
0x13 | Length of TLV data to follow | 2
0x14-0x15 | Data for this TLV |
0x16 | ACI Type 3 Message Indicators TLV ID | 0x13
0x17 | Length of TLV data to follow | 1
0x18 | Data for this TLV |
0x19 | Line Identity TLV ID | 4
0x1A | Length of TLV data to follow | variable 2 to 9, 9 = Default
0x1B-0x23 | Data for this TLV |
0x24 | Beginning of ACI Type 4 Message. Number of TLVs that follow | 4
0x25 | H0 H1 element TLV ID | 1
0x26 | Length of TLV data to follow | 2
0x27-0x28 | Data for this TLV |
0x29 | ACI Information Contained and Information Requested TLV ID | 0x0F
0x2A | Length of TLV data to follow | 2
0x2B-0x2C | Data for this TLV |
0x2D | Calling/Called Subscriber’s Basic Service Marks TLV ID | 0x12
0x2E | Length of TLV data to follow | 2
0x2F-0x30 | Data for this TLV |
0x31 | ACI Type 4 Message Indicators TLV ID | 0x14
0x32 | Length of TLV data to follow | 1
0x33 | Data for this TLV |
0x34 | Beginning of ACI Type 5 Message. Number of TLVs that follow | 3
0x35 | H0 H1 element TLV ID | 1
0x36 | Length of TLV data to follow | 2
0x37-0x38 | Data for this TLV |
0x39 | ACI Information Contained and Information Requested TLV ID | 0x0F
0x3A | Length of TLV data to follow | 2
0x3B-0x3C | Data for this TLV |
0x3D | Calling Subscriber’s Originating Facility Marks TLV ID | 0x15
0x3E | Length of TLV data to follow | 2
0x3F-0x40 | Data for this TLV |
0x41 | Beginning of ACI Type 6 Message. Number of TLVs that follow | 3
0x42 | H0 H1 element TLV ID | 1
0x43 | Length of TLV data to follow | 2
0x44-0x45 | Data for this TLV |
0x46 | ACI Information Contained and Information Requested TLV ID | 0x0F
0x47 | Length of TLV data to follow | 2
0x48-0x49 | Data for this TLV |
0x4A | Called Subscriber’s Terminating Facility Marks TLV ID | 0x16
0x4B | Length of TLV data to follow | 2
0x4C-0x4D | Data for this TLV |
0x4E | Beginning of ACI Type 7 Message. Number of TLVs that follow | 2
0x4F | H0 H1 element TLV ID | 1
0x50 | Length of TLV data to follow | 2
0x51-0x52 | Data for this TLV |
0x53 | ACI Information Contained and Information Requested TLV ID | 0x0F
0x54 | Length of TLV data to follow | 2
0x55-0x56 | Data for this TLV |
0x57 | Beginning of OLM Message. Number of TLVs that follow | 1
0x58 | H0 H1 element TLV ID | 1
0x59 | Length of TLV data to follow | 2
0x5A-0x5B | Data for this TLV |
0x5C | Beginning of SOO Message. Number of TLVs to follow | 1
0x5D | H0 H1 element TLV ID | 1
0x5E | Length of TLV data to follow | 2
0x5F-0x60 | Data for this TLV |
0x61 | Beginning of SEM Message. Number of TLVs to follow | 1
0x62 | H0 H1 element TLV ID | 1
0x63 | Length of TLV data to follow | 2
0x64-0x65 | Data for this TLV |
0x66 | Beginning of SIM Type 1 Message Number of TLVs to follow | 2
0x67 | H0 H1 element TLV ID | 1
0x68 | Length of TLV data to follow | 2
0x69-0x6A | Data for this TLV |
0x6B | Information Contained and Information Requested | 0x0F
0x6C | Length of TLV data to follow | 2
0x6D-0x6E | Data for this TLV |
0x6F | Beginning of SIM TYPE 2 Message Number of TLVs to follow | 6
0x70 | H0 H1 element TLV ID | 1
0x71 | Length of TLV data to follow | 2
0x72-0x73 | Data for this TLV |
0x74 | Information Contained and Information Requested | 0x0F
0x75 | Length of TLV data to follow | 2
0x76-0x77 | Data for this TLV |
0x78 | Facility Indicator Code | 0x1B
0x79 | Length of TLV data to follow | 2
0x7A-0x7B | Data for this TLV |
0x7C | Service Indicator Code | 0x1D
0x7D | Length of TLV data to follow | 2
0x7E-0x7F | Data for this TLV |
0x80 | Reserved Data Byte | 0x18
0x81 | Length of TLV data to follow | 1
0x82 | Data for this TLV |
0x83 | Line Identity (LI) | 4
0x84 | Length of TLV data to follow | Variable 2 to 9, 9 = Default
0x85-0x8D | Data for this TLV |
0x8E | Beginning of SIM TYPE 3 Message Number of TLVs to follow | 7
0x8F | H0 H1 element TLV ID | 1
0x90 | Length of TLV data to follow | 2
0x91-0x92 | Data for this TLV |
0x93 | Information Contained and Information Requested | 0x0F
0x94 | Length of TLV data to follow | 2
0x95-0x96 | Data for this TLV |
0x97 | Facility Indicator Code | 0x1B
0x98 | Length of TLV data to follow | 2
0x99-0x9A | Data for this TLV |
0x9B | Service Indicator Code | 0x1D
0x9C | Length of TLV data to follow | 2
0x9D-0x9E | Data for this TLV |
0x9F | Closed User Group Interlock Code | 0x1C
0xA0 | Length of TLV to follow | 4
0xA1-0xA4 | Data for this TLV |
0xA5 | Reserved Data Byte | 0x18
0xA6 | Length of TLV data to follow | 1
0xA7 | Data for this TLV |
0xA8 | Line Identity (LI) | 4
0xA9 | Length of TLV data to follow | Variable 2 to 9, 9 = Default
0xAA-0xB2 | Data for this TLV |
0xB3 | Beginning of SIM TYPE 4 Message Number of TLVs to follow | 4
0xB4 | H0 H1 element TLV ID | 1
0xB5 | Length of TLV data to follow | 2
0xB6-0xB7 | Data for this TLV |
0xB8 | Information Contained and Information Requested | 0x0F
0xB9 | Length of TLV data to follow | 2
0xBA-0xBB | Data for this TLV |
0xBC | Reserved Data Byte | 0x18
0xBD | Length of TLV data to follow | 1
0xBE | Data for this TLV |
0xBF | Line Identity (LI) | 4
0xC0 | Length of TLV data to follow | Variable 2 to 9, 9 = Default
0xC1-0xC8 | Data for this TLV |

Block 4

The L3P BT IUP configuration bytes below are included in Block 4.

Byte | Description of Block 4 Byte | Value
--- | --- | ---
0x01 | Yet more Data for this TLV |
0x02 | Beginning of SIM TYPE 5 Message Number of TLVs to follow | 7
0x03 | H0 H1 element TLV ID | 1
0x04 | Length of TLV data to follow | 2
0x05-0x06 | Data for this TLV |
0x07 | Information Contained and Information Requested | 0x0F
0x08 | Length of TLV data to follow | 2
0x09-0x0A | Data for this TLV |
0x0B | Facility Indicator Code | 0x1B
0x0C | Length of TLV data to follow | 2
0x0D-0x0E | Data for this TLV |
0x0F | Service Indicator Code | 0x1D
0x10 | Length of TLV data to follow | 2
0x11-0x12 | Data for this TLV |
0x13 | Reserved Data Byte | 0x18
0x14 | Length of TLV data to follow | 1
0x15 | Data for this TLV |
0x16 | Line Identity (LI) | 4
0x17 | Length of TLV data to follow | Variable 2 to 9, 9 = Default
0x18-0x20 | Data for this TLV |
0x21 | Six Character Network Address Extension | 0x1E
0x22 | Length of TLV data to follow | Variable 2 to 7 7 = Default
0x23-0x29 | Data for this TLV |
0x2A | Beginning of SIM TYPE 6 Message Number of TLVs to follow | 8
0x2B | H0 H1 element TLV ID | 1
0x2C | Length of TLV data to follow | 2
0x2D-0x2E | Data for this TLV |
0x2F | Information Contained and Information Requested | 0x0F
0x30 | Length of TLV data to follow | 2
0x31-0x32 | Data for this TLV |
0x33 | Facility Indicator Code | 0x1B
0x34 | Length of TLV data to follow | 2
0x35-0x36 | Data for this TLV |
0x37 | Service Indicator Code | 0x1D
0x38 | Length of TLV data to follow | 2
0x39-0x3A | Data for this TLV |
0x3B | Closed User Group Interlock Code | 0x1C
0x3C | Length of TLV data to follow | 4
0x3D-0x40 | Data for this TLV |
0x41 | Reserved Data Byte | 0x18
0x42 | Length of TLV data to follow | 1
0x43 | Data for this TLV |
0x44 | Line Identity (LI) | 4
0x45 | Length of TLV data to follow | Variable 2 to 9, 9 = Default
0x46-0x4E | Data for this TLV |
0x4F | Six Character Network Address Extension | 0x1E
0x50 | Length of TLV data to follow | Variable 2 to 7 7 = Default
0x51-0x57 | Data for this TLV |
0x58 | Beginning of SIM TYPE 7 Message Number of TLVs to follow | 3
0x59 | H0 H1 element TLV ID | 1
0x5A | Length of TLV data to follow | 2
0x5B-0x5C | Data for this TLV |
0x5D | Information Contained and Information Requested | 0x0F
0x5E | Length of TLV data to follow | 2
0x5F-0x60 | Data for this TLV |
0x61 | Facility Indicator Code | 0x1B
0x62 | Length of TLV data to follow | 2
0x63-0x64 | Data for this TLV |
0x65 | Beginning of SIM TYPE 8 Message Number of TLVs to follow | 5
0x66 | H0 H1 element TLV ID | 1
0x67 | Length of TLV data to follow | 2
0x68-0x69 | Data for this TLV |
0x6A | Information Contained and Information Requested | 0x0F
0x6B | Length of TLV data to follow | 2
0x6C-0x6D | Data for this TLV |
0x6E | Facility Indicator Code | 0x1B
0x6F | Length of TLV data to follow | 2
0x70-0x71 | Data for this TLV |
0x72 | Reserved Data Byte | 0x18
0x73 | Length of TLV data to follow | 1
0x74 | Data for this TLV |
0x75 | Line Identity (LI) | 4
0x76 | Length of TLV data to follow | Variable 2 to 9, 9 = Default
0x77-0x7F | Data for this TLV |
0x80 | Beginning of Send Service Message Number of TLVs to follow | 1
0x81 | H0 H1 element TLV ID | 1
0x82 | Length of TLV data to follow | 2
0x83-0x84 | Data for this TLV |
0x85 | Beginning of Service Message Number of TLVs to follow | 2
0x86 | H0 H1 element TLV ID | 1
0x87 | Length of TLV data to follow | 2
0x88-0x89 | Data for this TLV |
0x8A | Service Code TLV ID | 0x1F
0x8B | Length of TLV data to follow | 1
0x8C | Data for this TLV |
0x8D | Beginning of Suspend (SUS) Message Number of TLVs to follow | 2
0x8E | H0 H1 element TLV ID | 1
0x8F | Length of TLV data to follow | 2
0x90-0x91 | Data for this TLV |
0x92 | Reserved Data Byte | 0x18
0x93 | Length of TLV data to follow | 1
0x94 | Data for this TLV |
0x95 | Beginning of Resume (RES) Message Number of TLVs to follow | 2
0x96 | H0 H1 element TLV ID | 1
0x97 | Length of TLV data to follow | 2
0x98-0x99 | Data for this TLV |
0x9A | Reserved Data Byte | 0x18
0x9B | Length of TLV data to follow | 1
0x9C | Data for this TLV |
0x9D | Beginning of Repeat Attempt (RAM) Message Number of TLVs to follow | 1
0x9E | H0 H1 element TLV ID | 1
0x9F | Length of TLV data to follow | 2
0xA0-0xA1 | Data for this TLV |
0xA2 | Beginning of Re-answer (RAN) Message Number of TLVs to follow | 1
0xA3 | H0 H1 element TLV ID | 1
0xA4 | Length of TLV data to follow | 2
0xA5-0xA6 | Data for this TLV |
0xA7 | Beginning of SWAP Message Number of TLVs to follow | 3
0xA8 | H0 H1 element TLV ID | 1
0xA9 | Length of TLV data to follow | 2
0xAA-0xAB | Data for this TLV |
0xAC | Service Indicator Code | 0x1D
0xAD | Length of TLV data to follow | 2
0xAE-0xAF | Data for this TLV |
0xB0 | Reserved Data Byte | 0x18
0xB1 | Length of TLV data to follow | 1
0xB2 | Data for this TLV |
0xB3 | Beginning of Operator Override Message Number of TLVs to follow | 1
0xB4 | H0 H1 element TLV ID | 1
0xB5 | Length of TLV data to follow | 2
0xB6-0xB7 | Data for this TLV |
0xB8 | Beginning of Coin and Fee Checking Message Number of TLVs to follow | 1
0xB9 | H0 H1 element TLV ID | 1
0xBA | Length of TLV data to follow | 2
0xBB-0xBC | Data for this TLV |
0xBD | Beginning of Extend Call Message Number of TLVs to follow | 1
0xBE | H0 H1 element TLV ID | 1
0xBF | Length of TLV data to follow | 2
0xC0-0xC1 | Data for this TLV |
0xC2 | Beginning of Howler Message Number of TLVs to follow | 1
0xC3 | H0 H1 element TLV ID | 1
0xC4 | Length of TLV data to follow | 2
0xC5-0xC6 | Data for this TLV |
0xC7-0xC8 | Unused |

Block 5

The L3P BT IUP configuration bytes below are included in Block 5.

Byte | Description of Block 5 Byte | Value
--- | --- | ---
0x01-0x61 | Unused |
0x62-0x63 | Pointer to beginning of HLR TLVs | 4,0xC2
0x64-0x65 | Pointer to beginning of ECM TLVs | 4,0xBD
0x66-0x67 | Pointer to beginning of CFC TLVs | 4,0xB8
0x68-0x69 | Pointer to beginning of OOR TLVs | 4,0x63
0x6A-0x6B | Pointer to beginning of SWAP TLVs | 4,0xA7
0x6C-0x6D | Pointer to beginning of RAN TLVs | 4,0xA2
0x6E-0x6F | Pointer to beginning of RAM TLVs | 4,0x9D
0x70-0x71 | Pointer to beginning of RES TLVs | 4,0x95
0x72-0x73 | Pointer to beginning of SUS TLVs | 4,0x8D
0x74-0x75 | Pointer to beginning of SER TLVs | 4,0x85
0x76-0x77 | Pointer to beginning of Send Service TLVs | 4,0x80
0x78-0x79 | Pointer to beginning of SIM TYPE 8 TLVs | 4,0x65
0x7A-0x7B | Pointer to beginning of SIM TYPE 7 TLVs | 4,0x58
0x7C-0x7D | Pointer to beginning of SIM TYPE 6 TLVs | 4,0x2A
0x7E-0x7F | Pointer to beginning of SIM TYPE 5 TLVs | 4,2
0x80-0x81 | Pointer to beginning of SIM TYPE 4 TLVs | 3,0x63
0x82-0x83 | Pointer to beginning of SIM TYPE 3 TLVs | 3,0x8E
0x84-0x85 | Pointer to beginning of SIM TYPE 2 TLVs | 3,0x6F
0x86-0x87 | Pointer to beginning of SIM TYPE 1 TLVs | 3,0x66
0x88-0x89 | Pointer to beginning of SEM TLVs | 3,0x61
0x8A-0x8B | Pointer to beginning of SOO TLVs | 3,0x5C
0x8C-0x8D | Pointer to beginning of OLM TLVs | 3,0x57
0x8E-0x8F | Pointer to beginning of ACI TYPE 7 TLVs | 3,0x4E
0x90-0x91 | Pointer to beginning of ACI TYPE 6 TLVs | 3,0x41
0x92-0x93 | Pointer to beginning of ACI TYPE 5 TLVs | 3,0x34
0x94-0x95 | Pointer to beginning of ACI TYPE 4 TLVs | 3,0x24
0x96-0x97 | Pointer to beginning of ACI TYPE 3 TLVs | 3,9
0x98-0x99 | Pointer to beginning of ACI TYPE 2 TLVs | 2,0xBD
0x9A-0x9B | Pointer to beginning of ACI TYPE 1 TLVs | 2,0xA2
0x9C-0x9D | Pointer to beginning of CFN TLVs | 2,0x9A
0x9E-0x9F | Pointer to beginning of UBA TLVs | 2,0x95
0xA0-0xA1 | Pointer to beginning of BLA TLVs | 2,0x90
0xA2-0xA3 | Pointer to beginning of ULB TLVs | 2,0x8B
0xA4-0xA5 | Pointer to beginning of BLO TLVs | 2,0x86
0xA6-0xA7 | Pointer to beginning of CCF TLVs | 2.0x81
0xA8-0xA9 | Pointer to beginning of REL TLVs | 2,0x79
0xAA-0xAB | Pointer to beginning of CLR TLVs | 2,0x74
0xAC-0xAD | Pointer to beginning of ANS TLVs | 2,0x6C
0xAE-0xAF | Pointer to beginning of CAN TLVs | 2,0x61
0xB0-0xB1 | Pointer to beginning of TCM TLVs | 2,0x5C
0xB2-0xB3 | Pointer to beginning of CNG TLVs | 2,0x57
0xB4-0xB5 | Pointer to beginning of ACM TLVs | 2,0x4D
0xB6-0xB7 | Pointer to beginning of SASUI TLVs | 2,0x45
0xB8-0xB9 | Pointer to beginning of SAD TLVs | 2,0x3D
0xBA-0xBB | Pointer to beginning of SND TLVs | 2,0x35
0xBC-0xBD | Pointer to beginning of ASUI Type 2 TLVs | 2,0x1F
0xBE-0xBF | Pointer to beginning of ASUI Type 1 TLVs | 2,0x0B
0xC0-0xC1 | Pointer to beginning of FAM TLVs | 1,0xC0
0xC2-0xC3 | Pointer to beginning of SAM TLVs | 1,0xAC
0xC4-0xC5 | Pointer to beginning of IFAM TLVs | 1,0x88
0xC6-0xC7 | Pointer to beginning of IAM TLVs 0xC6 contains Block Number 1, 2, 3, 4, or 5 0x67 contains the offset to the byte within the block. Range 1 to 0xC8 | 1, 0x64

See Programmable Protocol Language.
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Integrated Services Digital Network.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
Interworking is a software feature within the Excel platform call control layer that enables protocol conversion by analyzing and converting Network Signaling (NS) Layer 3 information.
See Information Control Block.
See Request For Service.
Destination Point Code
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Blocking Acknowldgment message
Random Access Memory
See Recorded Announcements.