0x02C3 Gatekeeper Auto Registration

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x2C3 Auto Registration
2, 3 | Length 0x0002
4, 5 | Value[0, 1] Auto Registration 0x0000 Disabled (Default) 0x0001 Enabled

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).