You are here: SwitchKit® Development Environment - CSA User’s Guide > 7 System Provisioning and Monitoring > Performing an Ethernet Redundancy SwitchOver

Performing an Ethernet Redundancy SwitchOver

Right-click the DSP-S2 card and select the menu option, SwitchOver Ethernet Redundancy.

Next, a warning message appears.

If you select Yes, then the next dialog box opens. Select the port for which the switchover is to be performed. Note that the current active port is disabled in the dialog box.

If you select the port and click OK, a message confirms ethernet redundancy is enabled on the port, indicating the switchover was successful.

Digital Signal Processor
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.