You are here: CSP Developer’s Guide: Common Channel Signaling > 8 ISDN > ISDN Over Ethernet

ISDN Over Ethernet

Overview

Prior to this feature, the communication between the ISDN Series 3 card and the CSP Matrix Series 3 Card used the mid-plane HDLC bus. Communication over the HDLC bus slows the maximum number of messages that can be transmitted to be less than 100 per second, not allowing the user to achieve high call rates that require ISDN services.

Using Ethernet communication for messaging between a ISDN Series 3 card and CSP Matrix Series 3 Card allows increased performance by providing more message transactions per second.

This feature supports a new RCOMM state machine on the ISDN Series 3 card that monitors the status of the link between this card and CSP Matrix Series 3 Card. Communication over the HDLC bus will continue to be supported. Licensing of this feature is not required.

Description

When using the Ethernet communication mode, all the I/O ports are connected to the same physical Ethernet switch/hub. Redundancy at the port level is provided by the RCOMM state machine that monitors the status of the link between the ISDN Series 3 and Matrix Series 3 ports. The message packets are sent out of the port which indicates a link-up state. Additional logic provides a fall-back to the HDLC option in the event of a failure of all the Ethernet ports.

ISDN Series 3 Card and CSP Matrix Series 3 Card Ethernet Interconnections

API Alarm Monitoring

The Alarm (0x00B9) message supports the new 0x02 Card Alarm, 0x52 ISDN Ethernet Unavailable:

• If at any point the message communication mode is changed from Ethernet to the HDLC bus, an alarm is sent to the host.

• An Alarm Cleared (0x00C1) message is sent if the communication mode is changed back to the Ethernet mode.

See Integrated Services Digital Network.
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.
In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.