0x011A Call Agent Mode Physical Channel ID

Used in:
0x1E Generic PPL ICB in:
PPL Event Request message
Connect with Data message

Byte | Description
0, 1 | Tag 0x011A - Call Agent Mode Physical Channel ID
2, 3 | Length 0x0003
4,5 | Value[0, 1] Span ID
6 | Value[2] Channel ID

See Programmable Protocol Language.
See Information Control Block.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.