You are here: CSP Hardware Product Descriptions > 4 Common Channel Signaling Cards > Dialogic® Signaling System #7 Series 3 Card - See Model Numbers

Dialogic® Signaling System #7 Series 3 Card - See Model Numbers

Description

The Dialogic® Signaling System #7 Series 3 card provides Signaling System 7 services for the CSP fully integrating switching and advanced signaling applications. The SS7 Series 3 card enables the CSP to act as a Signaling Point (SP) in the SS7 network architecture.

Microprocessor

The SS7 Series 3 card is a Power PC-based SS7 controller card.

Redundancy

You achieve redundancy by installing, connecting and configuring a pair of SS7 Series 3 cards. Refer to the CCS I/O Series 3 card Hardware Product Description for more information on redundancy.

Placement

Each CSP 2090, CSP 2110 or CSP 2040 chassis can accommodate SS7 Series 3 cards which reside in the front slots.

Configuration Information

The part number, serial number, model number, and revision are located on the back of the board.

Specifications

The SS7 Series 3 card is designed to the following electrical, physical and environmental specifications.

Electrical | Specification
--- | ---
Supply Voltage, Vcc | 5.00V
Supply Current, Vcc @ 5.0V | 4.73A (typical)

Physical | Specification
--- | ---
Height | 236.2 mm (9.3 in.)
Depth | 317.5 mm (12.5 in.)
Width | 19.7 mm (0.775 in.)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

SS7 Series 3 Card Models

The available SS7 Series 3 card models are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
SS7 Line Card, 2 Link | CSP-SS7-1302 | CSP-SS7-1302R
SS7 Line Card, 4 Link | CSP-SS7-1304 | CSP-SS7-1304R
SS7 Line Card, 6 Link | CSP-SS7-1306 | CSP-SS7-1306R
SS7 Line Card, 8 Link | CSP-SS7-1308 | CSP-SS7-1308R
SS7 Line Card, 10 Link | CSP-SS7-1310 | CSP-SS7-1310R
SS7 Line Card, 12 Link | CSP-SS7-1320 | CSP-SS7-1320R
SS7 Line Card, 14 Link | CSP-SS7-1340 | CSP-SS7-1340R
SS7 Line Card, 16 Link | CSP-SS7-1360 | CSP-SS7-1360R

Related Products

The products related to the SS7 Series 3 card are listed below.

Product | Model No. | Model No.
--- | --- | ---
CCS I/O Series 3 Card | EXS-7IO-1300 | EXS-7IO-1300R
CCS I/O Series 3 Redundancy Cable | Part No. 64-3333-00 | Part No. 64-3333-00

Front View

The front view shows the LEDs, push button switches and Monitor connector.

Controls and Indicators

The table below describes the LEDs and push button switches as shown in the front view of the card.

LED | Color/Status | Description
--- | --- | ---
Diag | Green | This LED is green except during a card reset when this LED goes out briefly. This LED is normally OFF.
Red | Redundancy has been configured.
Off | No diagnostics running
Status | Green | The card is connected to the system buses.
Red | The Stop push button has been pressed. The card is disconnected from the system buses.
Off | Not applicable.
Halt | Green | The CPU is running.
Red | The CPU has halted. This LED is red briefly during card reset.
Off | CPU hard reset
Power | Green | Good power
Off | Bad power
Push Buttons | Description |
Stop | Removes card from the system buses. Always press the Stop push button before removing the card from the chassis.
Stop and S Reset together | Initiates a Hard Reset. The Flash and SDRAM are reset, as is the processor and all of its internal registers. A Hard Reset also occurs when the Watchdog times out twice in a row.
S Reset | Initiates a Soft Reset. The code running on the processor is reset, and the Flash is put into a read state.

DIP Switch SW1

The table below describes the DIP switch SW1 settings. The shading (asterisk* for html documents) indicates factory-installed settings.

Position | Setting | Function
--- | --- | ---
1 | ON* | Disables Debug 1 Mode
OFF | Enables Debug 1 Mode
2 | ON* | The Monitor port setting is 19200 baud.
OFF | The Monitor port setting is 19200 baud.
3 | ON* | Disables Debug 2 Mode
OFF | Enables Debug 2 Mode
4 | ON* | Ethernet Link, Auto-Negotiate Mode (Default)
OFF** | Ethernet Link, Force 100 Mbps/Full Duplex Mode
5 | ON* | Reserved, normally should be ON
OFF | Reserved
6 | ON* | Reserved, normally should be ON
OFF | Reserved
7 | ON* | Reserved, normally should be ON
OFF | Reserved
8 | ON* | Reserved, normally should be ON
OFF | Reserved

** Enables Ethernet Link, Force 100 Mbps/Full Duplex feature.

Jumpers

The table below indicates the jumper settings.

Jumper | Setting | Description
--- | --- | ---
JP1 | Installed (default) | Factory use only
JP2 | Installed (default) | Factory use only
JP3 | Installed (default) | Factory use only
JP4 | Not Installed (default) | Hardware Watchdog Timer enabled
JP5 | Installed (default) | Factory use only
JP7 | Not Installed (default) | Factory use only
JP8 | Installed (default) | Factory use only
JP9 | Installed (default) | Factory use only
JP10 | Installed (default) | Factory use only
JP11 | Installed (default) | Factory use only

Side View

The side view shows DIP switch SW1 and jumper JP4.

SS7. A common channel signaling protocol providing supervision, alerting, and addressing services.
See Signaling System Number Seven.
Signaling Point
See Common Channel Signaling.
Quick depress and release of the phone plunger of a handset to signal the PBX or Centrex of instructions to follow (e.g., Call Transfer).
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.