0x2A0A Media Payload Size

SIP

Used in:
0x0033 NPDI Universal ICB

Byte | Description
0, 1 | Tag 0x2A0A
2, 3 | Length 0x0002
4 | Value Packet Duration in milliseconds

Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.
Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.