0x0269 Use SIP T2 Timer

Use this TLV to specify the T2 timer value in milliseconds. The default value is 0xFA0 (4000 milliseconds).

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x0269
2, 3 | Length 0x0004
4-7 | Value[0-3] T2 Timer (4 Bytes)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).