0x1C SS7 TUP Formatted Fields

Used in:
Channel Release Request, Channel Released With Data, Connect With Data, Release Channel with Data, Route Control, Outseize Control, PPL Event Indication, PPL Event Request messages.

ICB Type | 0x02 (Data)
ICB ID | 0x1C
Data Length | Variable
Data[0, 1] | TUP Message Group/Type
Data[2] | Number of Fields (variable)
Data[3] | Field 1 ID (Refer to the TUP Message Format Configure message)
Data[4] | Field 1 Data Length (variable)
Data[5] | Field 1 Data[0]
Data[:] | Field n ID (Refer to the TUP Message Format Configure message)
Data[:] | Field n Data Length (variable)
Data[:] | Field n Data[0]

Outgoing call setup during real-time call processing on a specific channel.
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.
Telephone User Part