0x0026 Channel Pad Value

Used in:
Connect with Data message

ICB Type | 0x02
ICB ID | 0x26 ISDN Segmented Message
Data Length | 0x02
Data[0] | Channel A Pad Value The dB gain/loss adjustment of the signal transmitted to Channel A 0x00 +3 dB Gain/Loss 0x01 0 dB 0x02 2 dB 0x03 3 dB 0x04 4 dB 0x05 6 dB 0x06 9 dB
Data[1] | Channel B Pad Value The dB gain/loss adjustment of the signal transmitted to Channel B 0x00 +3 dB Gain/Loss 0x01 0 dB 0x02 2 dB 0x03 3 dB 0x04 4 dB 0x05 6 dB 0x06 9 dB

See Information Control Block.