0x0601 NFS Poll Retries

Use this TLV in the Generic Card Configure message to set the number of polls the NFS server can miss before being marked out of service.

Byte | Description
0, 1 | Tag: 0x0601 - NFS Poll Retries
2, 3 | Length: 0x0004
4, 5 | Value[0, 1]: NFS Poll Retries: Default = 0x0001
6, 7 | Value[2, 3]: NFS Read Retries: Default = 0x0003 (not configurable)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.