ISUP CVS Configuration Bytes (ANSI)

Byte | Description | Value
--- | --- | ---
0x01 | CIN | 0x00=Not Configured 0x01=Configured (default)
0x02 | CLLI | 0x00=Not configured 0x01=Configured (default)
0x03 | CVR Processing | 0x00=Do Not Process/Send PPL Event (default) 0x08 (CVR Received) to Host 0x01=Send CVR
0x04 (Continued on next page) | CGC Indicator | 0x00 (default) Bits 1, 0=Circuit Group Carrier Indicator 00=Unknown 01=Analog 10=Digital 11=Digital and Analog. Bits 3, 2=Double Seizing Indicator 00=Always 00; configuration is taken from CPC data. DO NOT CHANGE.
0x04 (Continued) | CGC Indicator | Bits 5, 4=Alarm Carrier Indicator 00=Unknown 01=Software Carrier Handling 10=Hardware Carrier Handling 11=Spare Bits 7, 6- Continuity Check Requirement Indicator 00=Unknown; 01=None; 10=Statistical; 11=Per Call
0x05-0x06 | Unused |
0x07 | Timer to be used by UPU/CVT Test | 0–24 Timer 2 (30s) (default)
0x08 | CVT Re-attempt Count | 0–255 8 (default)
0x09 | Unused |

For CLLI and CIN parameter formats, refer to ANSI T1-113.

See Programmable Protocol Language.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)