0x068D Transit Connection Mode

Use this TLV with the DSP Chip AIB in the following message to set the conference one-way (input only) temporarily, while the tone/file is being played.

• Resource Create (0x0124)

• Resource Connect (0x0127)

Byte | Description
0, 1 | Tag: 0x068D Transit Connection Mode
2, 3 | Length: 0x0002
4-5 | Value [0,1] onference leg connection behavior while transmitting tone/file 0x0000: Remove leg (Default) 0x0001: Connect Input Only

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor
See Address Information Block.