You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > IP Signaling Series 3 Card Status Report 0x0105

IP Signaling Series 3 Card Status Report 0x0105

Type

EXS API message

Description

IP Signaling Series 3 Card Status Report 0x0105

This message is sent unsolicited from the IP Signaling Series 3card to the host in different scenarios. This is generally caused by some Matrix interaction of which the host requires notification.

Sent by

CSP

EXS Hex API Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0xNNNN)
3, 4 | Message Type (0x0105) | 3, 4 | Message Type (0x0105)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Sequence Number (same as message)
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | : | AIB Same as message
Number of AEs to follow
AEs 0x48 Ring Communication Link 0x53 Object Type
: | Number of TLVs to Follow 0x01 | : | Checksum
: | TLV 0x0020 IP Signaling Series 3 Card Interface Status |  |
: | Checksum |  |

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.