L3P MGR Configuration Bytes

Byte | Description | Values (* Default)
--- | --- | ---
0x01 | BCC Clear all calls or do not clear all calls when both C Channels are dead when switchover failure occurs. | *0x00 = BCC Clear All Calls 0x01 = BCC Do not clear all calls
0x02 | PCM Encoding Format | 0x01 = MU Law Encoded PCM *0x02 = A Law Encoded PCM 0x03 = Mixed Encoded PCM 0x01 = DS2 A Law Encoded PCM
0x03 | Wait for Startup Request from host, when Layer Manager receives Startup Fail from System Management | *0x00 = Do not wait 0x01 = Wait
0x04 | Type of Port Alignment Important! When this Config Byte is set to 2, the other side must be intelligent enough to send block indications to the ports that are locally blocked. | 0x00 = Unblock all user ports, then block locally-blocked ports *0x01 = Perform accelerated port alignment procedure, then block locally-blocked ports 0x02 = Block locally-blocked ports
0x05 | Send Reset Sequence Number during startup procedure | *0x00 = Do not send 0x01 = Send
0x06 | Send all Status Indications to the host | *0x00 = Send only relevant Status Indications 0x01 = Send all Status Indications (used for diagnostics purposes only)
0x07 | Enable Port Alignment Procedure | 0x00 = Disabled (LE default) *0x01 = Enabled (AN default)
0x08 | Link blocking action after startup | 0x00 = Do not send block or unblock links (links will default to operation for the first startup) *0x01 = Send block link only for links that are locally blocked 0x02 = Send both unblock or block for all links depending on previous link status
0x09 | Layer Manager Mode | *0x00 = Non-protective Mode 0x01 = Protective Mode

See Pulse Code Modulation.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."