You are here: CSP Developer’s Guide: Line Cards > 3 J1 Information > J1 Supported Features

J1 Supported Features

This CSP supports the following features:

• Clear Channel for 30 J-ONE channels

• A maximum of four J-ONE cards per CSP

• 16 spans per J-ONE card

• 30 ports per J-ONE span (480 ports per card)

Signaling technique where the full channel bandwidth is used for data transmission, while the framing and control bits (signaling) use a separate channel. No control or signaling is performed on this path. See B8ZS and ZBTSI.