You are here: CSP Developer’s Guide: Overview > 3 Getting Started > Robust Ethernet Redundancy

Robust Ethernet Redundancy

Alarm

This feature improves alarming and CSP reporting of Ethernet switch-overs. When the Ethernet ports are in redundant mode and an Ethernet switchover occurs, the CSP sends the Ethernet Switchover Occurred alarm (Card Alarm 0x4F) to the host. Refer to the Alarm Message (0x00B9) in the API Reference.

Unsolicited Reports

The CSP also send the following messages without the host requesting them:

• The active Ethernet interface is reported in every AB Poll. Refer the Card Status bit mask in the Poll (0x00AB) message in the API Reference.

• Whenever the CSP issues a Card Status Report for the Matrix Controller I/O, the report contains an indication of the active interface and each interface’s link detect state.

Selecting Active Ethernet interface

Use the IP Address Configuration message to select the active Ethernet interface. Refer to this message in the API Reference.

Do not use this message while the CSP is passing data. Doing so could result in data loss

Querying

Use the IP Address Configure Query (0x00E6) message to query which Ethernet Interface is active.

CSA

Refer to the CSA User’s Guide for instructions on Querying and Switching Over Ethernet Redundancy.

The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
See Converged Services Administrator.