SSUTR2 CPC PPL Timers

Timer ID | Timer | Default Value (10ms)
--- | --- | ---
0x01 | Wait for subsequent address message Tsam | 1500
0x02 | Release guard timer1 Tlig | 1000
0x03 | Release guard timer2 T(FIU repeat) | 6000
0x04 | Wait for 1st backward signal timer Tacf | 2400
0x05 | Non receipt of reply signal Triu | 24000
0x06 | Non receipt of FIU after sending clearback Tfiu | 3000
0x07 | Non hang-up of the caller after receipt of a hang-up signal of the called subscriber | 500
0x08 | Non receipt of continuity test message Tcont | 1500
0x09 | Non receipt of the end signal after transmission of a call setup failure signal | 1000s
0x0A | ECH repetition stop T(ECH, repeat) | 6000