0x01ED RFC 2833 Jitter Buffer Size

Indicates the size of the RTP jitter buffer in milliseconds. The range is 0-400 milliseconds. The default is 200 milliseconds.

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x01ED
2, 3 | Length 0x0002
4, 5 | Value[0] Value in milliseconds. 0x0000-0x0190 (0-400 ms) 0x00C8 (200 ms) is the default

Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).