0xE003 AIB Container TLV

Used in the Resource Delete Indication message (0x0129) when deleting a child conference

Byte | Description
0, 1 | Tag 0xE003
2, 3 | Length 0x0008
4 | Value[0] Address Method 0x00 (Single Entity)
5 | Value[1] Address Element Count 0x01
6 | Value[2] Address Element 0x45
7 | Value[3] Data Length 0x04
8, 9 | Value[4, 5] Parent Conference ID
10, 11 | Value[6, 7] Child Conference ID

The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.