You are here: CSP Developer’s Guide: Overview > 8 DSP Series 2 Cards Product Description > Default Transmit Call Progress Tones

Default Transmit Call Progress Tones

Default transmit call progress tones shows the default tones that the CSP uses to generate call progress tone patterns. Each call progress tone is distinguished by an ID. Note that some of the tones are single frequencies, while others are combinations of frequencies, at specific dBm levels.

You can modify any of the default tones shown in the table below, but you cannot create a new Tone ID. The tone that was originally associated with that Tone ID becomes unavailable and the change affects all patterns that use that tone.

Table 8-10 Default transmit call progress tones

|  | Tone ID
--- | --- | ---
Specification | 00 | 01 | 02 | 03 | 04 | 05 | 06 | 07 | 08 | 09 | 0A | 0B | 0C
Frequency Count | 0 | 1 | 1 | 2 | 2 | 2 | 4 | 1 | 1 | 1 | 1 | 1 | 1
Frequency 0 (Hz) |  | 440 | 480 | 350 | 440 | 480 | 1,400 | 914 | 985 | 1,371 | 1,429 | 1,777 | 400
dBm 0 |  | -15 | -15 | -15 | -20 | -20 | -8 | -13 | -13 | -13 | -13 | -13 | -18
Frequency 1 (Hz) |  |  |  | 440 | 480 | 620 | 2,060 |  |  |  |  |  |
dBm 1 |  |  |  | -15 | -20 | -20 | -8 |  |  |  |  |  |
Frequency 2 (Hz) |  |  |  |  |  |  | 2,450 |  |  |  |  |  |
dBm 2 |  |  |  |  |  |  | -8 |  |  |  |  |  |
Frequency 3 (Hz) |  |  |  |  |  |  | 2,600 |  |  |  |  |  |
dBm 3 |  |  |  |  |  |  | -8 |  |  |  |  |  |

Hertz