MTP3 HMDT PPL Event Requests

Event ID | Event
--- | ---
0x01 | Start or restart interval reporting. If restarting the measurement interval, this event will result in reports for the current measurement interval before restarting.
0x02 | Stop interval reporting. Immediately stop interval reporting.

In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.