You are here: CSP Developer’s Guide: Internet Protocol > 5 Session-Initiation Protocol (SIP) Software > SIP Redundancy

SIP Redundancy

This section describes SIP Redundancy including the following two features:

• Dual Ethernet Port

• SIP User Agent Redundancy

Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.