You are here: SwitchKit® Development Environment - CSA User’s Guide > 2 Basic Configuration - System/Node > Updating or Deleting a Node Online or Offline

Updating or Deleting a Node Online or Offline

This procedure describes how to update or delete a node within the CSA graphical user interface when the CSA is connected to a CSP or not connected.

Before you begin

Updating

If the node to be updated is online, you must already have system software downloaded through a TFTP server. The LLC and SwitchManager must be running. For information on starting the LLC and SwitchManager refer to the SwitchKit documentation set.

Deleting

If the node to be deleted is online you must already have system software downloaded through a TFTP server. The LLC and SwitchManager must be running. For information on starting the LLC and SwitchManager refer to the SwitchKit documentation set.

If you already have other nodes configured, selecting the menu option Configuration® Configure Through SwitchMgr® Send All Configurations To Switch will reconfigure those nodes. Thus, Send All Configurations To Switch should only be used when creating a new configuration. Send All Configurations To Switch replaces any previous configuration. When updating or deleting a node in an already configured system, you should select the menu option Configuration® Configure Through SwitchMgr® Send Only Modified Configuration To Switch.

Steps for Updating or Deleting a Node

Do the following to update or delete a node online or offline.

1 Go to the global view and do one of the following:

• Right-click the configuration icon and select IP Address Configuration.

• Click on the configuration icon and then on the menu select Configuration®Change IP Address/Node ID.

• Click on the configuration icon and then on the menu select Configuration®System® IP Address Configuration.

• Go to the configuration node view, right-click in the blue area around the slots and select Change IP Address/Node ID.

The Configure Node... dialog box opens.

2 To update the node, you may enter a new IP address, logical node ID or node type. Then click OK.

To delete the node, in the Action field, select Delete Node from the drop-down list. Then click OK.

Note

Configuration changes are not sent to the CSP until you select the menu: Configuration®Configure Through SwitchMgr ®Send Only Modified Configuration To Switch.

See Converged Services Administrator.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).