You are here: SwitchKit® Development Environment - CSA User’s Guide > 7 System Provisioning and Monitoring > Enable Ethernet Redundancy

Enable Ethernet Redundancy

Right-click the DSP-S2 card and select the menu option, Enable Ethernet Redundancy.

If redundancy is disabled and you select to enable redundancy, the next dialog box opens:

Select the port you want to use for Ethernet redundancy in the next dialog box and then click OK..

The node view will then confirm that Ethernet redundancy is enabled. This is indicated in the next message:

If you select a port that is not available, the next available port is automatically selected. If no ports are available the next message appears:

Digital Signal Processor
The protocol used in most local area PC networks. Typically, most Ethernet networks support data transmission speeds up to 10 Mbps, but 100 Mbps is also possible.