0x904E Signaling Gateway Process Query

Used in:
NGA Configure Query message

Byte | Description
0, 1 | Tag 0x904E
2, 3 | Length Variable
4,5 | Value[0] Port
6 | Value[2] Number of IP addresses
7-10 | Value[3-6] IP Address (4 bytes)
: | Value [:]
: | Value[:] IP Address (4 bytes)

The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).