You are here: CSP Hardware Product Descriptions > 1 Chassis > CSP Blockout Cards and Panels - See Part Numbers

CSP Blockout Cards and Panels - See Part Numbers

Description

Blockout cards and panels are required in the CSP 2090, CSP 2110, and CSP 2040 chassis to ensure proper air flow and cooling.

Front Blockout Cards

Install Front Blockout cards in all unoccupied card slots in the front of the chassis.

Rear Blockout Cards

Install Rear Blockout cards in all unoccupied I/O card slots in the rear of the chassis.

Power Blockout Panel

Install a Power Blockout panel over unused Power card slots.

Specifications

The blockout cards and panel are designed to the following physical specifications.

Front Blockout Card | Specification
--- | ---
Height | 208.3 mm (8.2 in.)
Depth | 309.9 mm (12.2 in.)
Width | 14.5 mm (0.57 in.)

Rear Blockout Card | Specification
--- | ---
Height | 288.3 mm (11.35 in.)
Depth | 98.6 mm (3.88 in)
Width | 14.5 mm (0.57 in.)

Power Blockout Panel | Specification
--- | ---
Height | 236.2 mm (9.3 in.)
Width | 31.8 mm (1.25 in.)

Part Numbers

The Blockout card and panel part numbers are listed below.

Product | Part Number
--- | ---
CSP Front Blockout Card | 71-0270-02
CSP Rear Blockout Card (I/O) | 71-0271-02
CSP Power Blockout Card | 71-0506-00

Related Products

The products related to the Blockout cards and panel are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
CSP 2040 Chassis | CSN-CHA-1112 | CSN-CHA-1112R
CSP 2090 Chassis | EXS-CHA-1100 | EXS-CHA-1100R
CSP 2110 Chassis | EXS-CHA-1201 | EXS-CHA-1201R

Views

The following views show the Blockout cards and panel.