0x000B V5 Cpath Assignment

Used in:
V5 Configure message
V5 Configuration Query message

This TLV is currently not supported.

Byte | Description
0 | Tag 0x00 V5 Cpath Assignment (MSB)
1 | Tag 0x0B V5 Cpath Assignment (LSB)
2 | Length 0x00 (MSB)
3 | Length 0x02 (LSB)
4 | C Channel ID
5 | Cpath Type 0x00 = PSTN

Before adding a C path you must create a C Channel and the C Channel should belong to Protection Group 2. Protection Group 2 is not supported.

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Most Significant Bit
Least Significant Bit
Public Switched Telephone Network