ISUP CVR Configuration Bytes (ANSI)

For the CLLI and CIN parameter formats in the table below, refer to ANSI T1-113.

Byte | Description | Value
--- | --- | ---
0x01 | CLII | 0x00=Not Configured 0x01=Configured (default)
0x02 | CIN | 0x00=Not configured 0x01=Configured (default)
0x03 | CGC Indicator | 0x00 (default) Bits 1, 0=Circuit Group Carrier Indicator 00=Unknown 01=Analog 10=Digital 11=Digital and Analog. Bits 3, 2=Double Seizing Indicator 00=Always 00; configuration taken from CPC data. DO NOT CHANGE Bits 5, 4=Alarm Carrier Indicator 00=Unknown 01=Software Carrier Handling 10=Hardware Carrier Handling 11=Spare Bits 7, 6- Continuity Check Requirement Indicator 00=Unknown; 01=None; 10=Statistical; 11=Per Call
0x04 | Message ID | 0xEB (CVR)
0x05 | Number of Mandatory Parameters | 2 (default)
0x06 | CVR Indicator Parameter Code | 0xE6
0x07 | CVR Indicator Parameter Length | 0x01
0x08 | CGC Parameter Code | 0xE5
0x09 | CGC Parameter Length | 0x01
0x55 | CVT Indication to host | 0x00=Disable (default) 0x01=Enable

American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)