0x027E SIP Persistent Sockets

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

This TLV forces all TCP sockets to be persistent.

Byte | Description
0, 1 | Tag 0x027E
2, 3 | Length 0x0001
4-7 | Value[0-3] 0 disable (default) 1 enable

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.