0x0600 NFS User Group ID

Use this TLV in the Generic Card Configure message if you want to modify the default NFS User Group ID information. You should send this TLV at the same time you are configuring the card for NFS (along with the File Management Configure TLV).

Byte | Description
0, 1 | Tag: 0x0600 - NFS User Group ID
2, 3 | Length: Variable
4, 5 | Value[0, 1]: User ID (Default is 2001)
6, 7 | Value[2, 3]: Group ID (Default is 100)
8, 9 | Value[4, 5]: Local Name Length
10 . . . | Value[6 . . . ]: Local Name

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.