L3P CIC PPL Event Indications (ITU)

The following table shows the PPL Event Indications supported by ITU ISUP L3P CIC.

Event ID | Event
--- | ---
0x01 | Reset circuit success indication
0x08 | Remote maintenance block or maintenance group block indication
0x09 | Remote maintenance unblock or maintenance group unblock indication
0x0A | ACM received
0x0B | ANM received
0x0C | CPG received
0x0E | ISUP protocol violation
0x0F | Remote hardware group block indication
0x10 | Remote hardware group unblock indication
0x11 | CON received
0x12 | Local maintenance block / group maintenance block success
0x13 | Local maintenance unblock / group maintenance unblock success
0x15 | Local circuit maintenance unblocking indication
0x16 | UCIC received
0x19 | OLM received
0x32 | SGM message received
0x5A | SAM wait timer expired. The CSP receives an inbound call (IAM) and checks to see if the Request for Service message in the IAM is enabled (component 0x000F, byte 0x30 is set to 1). If so, the CSP checks if the number of maximum digits has been received (set in byte 0x31) and if it is not exceeded the CSP looks for the "f" digit in the called party number (or whatever is set in byte 0x32). If the maximum has not been received and the "f" was not included in the called party number the CSP starts timer 0x05 (component 0x000F) which is set to four seconds by default (unless changed in the configuration file). Upon expiration of Timer 0x05, this indication is sent to the host and then the RFS message is sent to the host.
0x63 | DSP Resource Allocation Failure

See Programmable Protocol Language.
International Telecommunications Union (UN)
See Integrated Services Digital Network User Part.
See Circuit Identification Codes.
See Request For Service.
Digital Signal Processor