SSUTR2 SPRC Configuration Bytes

Byte | Description | Value
--- | --- | ---
0x01 | SIO subservice field | 8
0x02 | SIO service indicator | 4
0x0A | Pause/Resume option | 0
0x28 | Number of samples, n, in moving average | 100
0x29 | Instantaneous Onset Threshold for Incoming Calls, 100 ms units | 100 ms
0x2A | Moving Average Onset Threshold for Incoming Calls, 100 ms units | 50 ms
0x2B | Abatement Threshold for Incoming Calls, 100 ms units | 10 ms
0x2C | Number of samples, x, received before clearing congestion condition for Incoming Calls | 10
0x2D | Instantaneous Onset Threshold for Outgoing Calls, 100 ms units | 100 ms
0x2E | Moving Average Onset Threshold for Outgoing Calls, 100 ms units | 50 ms
0x2F | Abatement Threshold for Outgoing Calls, 100 ms units | 10 ms
0x30 | Number of samples, x, received before clearing congestion condition for Outgoing Calls | 10