You are here: CSP Developer’s Guide: Overview > 7 Configuring and Using Resources on the DSP Series 2 Cards > Connecting to an ASR with Positive Voice Detection

Connecting to an ASR with Positive Voice Detection

Introduction

NOTE: This feature is not supported in this release.

If you have enabled RTP with the Positive Voice Detection (in the Record File Start 0x011E message), you would start/stop sending RTP packets using the Record File Modify 0x011F message with the following TLVs:

• 0x0689 - Start/Stop Sending RTP Packets

• 0x068A - Calender Time Offset for Sending RTP Packets

Pre-requisite

You must have Positive Voice Detection enabled and implemented. See Implementing Positive Voice Detection/Answering Machine Detection.

Message Sequence

Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.